RTI CX10 Firmware Version 22.3.31

VERIFYING THAT YOU NEED THE UPGRADE
If you already have version 22.3.31 or newer you should not upgrade your
firmware to this version. Use the "Get Firmware Version" command from
the Communications menu in TheaterTouch Designer or Integration Designer
to determine the current firmware version. The reported version number
will consist of a number followed by a bootloader version number
[for example: 22.3.31 (Bootloader: 1.5)]. If the first part of the reported
version number is 22.3.31 or higher, you do not need this update.

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
TheaterTouch Designer 3.0 or higher, or Integration Designer 6.0 or
higher must already be installed on the PC that you wish to use to
upgrade the CX10 firmware.  If your PC runs a 64-bit version of Windows,
Integration Designer 7.0 must be installed to perform the upgrade.
Upgrading to the latest version of Integration Designer is strongly
recommended.  You should verify that you can communicate with the CX10
using Integration Designer before attempting to upgrade the firmware.

FIRMWARE UPGRADE PROCEDURE
1. Connect power to the CX10 and make sure it operates normally.
2. Make sure Integration Designer 6.0 or higher is installed on the
   PC that you are using to update the CX10 firmware, and that Integration
   Designer can communicate successfully with the CX10. You can use the
   "Get Firmware Version" command on the Communications menu in Integration
   Designer to verify that the USB communications are working properly.
3. Run the .exe program contained in this ZIP file and follow
   the on-screen instructions carefully.

LIST OF CHANGES IN THIS RELEASE (RELEASE 22.3.31)
- Add support for switching multiple camera feeds on a single RTSP object
- Add additional fonts
- Change system variable handling so that only unique variables count against
  the per-page limit instead of every use of the same variable

LIST OF CHANGES IN RELEASE 20.11.20
- Preserve the system name during firmware upgrades. 
- Allow use of WiFi channels 12 & 13 in countries that support them.
- Add support for BMP-format dynamic images.
- Improved VoIP SIP registration.
- Add Hebrew, Arabic and right-to-left font support.

LIST OF CHANGES IN RELEASE 20.8.25
- Improved reliability of the system file downloads and firmware upgrades
- Improved network reliability in certain environments
- Fixed intermittent dynamic image loading over SSL
- Improved overall system performance

LIST OF CHANGES IN RELEASE 2.0.5
- Improved reliability of Firmware Updates and System Downloads.
- Fixed firmware updates from computers with multiple network adapters.
- Prevented CX-10 from getting into a continuous boot cycle.
- Fixed Composite Video for PAL

LIST OF CHANGES IN RELEASE 1.2.11
- Added RTSP/H.264 streaming support
- Fixed misc. VoIP issues
- Improved PNG decoding reliability

LIST OF CHANGES IN RELEASE 1.1.5
- Added the ability to update firmware over the network
- Improved image decoding reliability (GIF,PNG,JPG)