RTI ISR-2 and ISR-4 Firmware Version 25.10.30


FIRMWARE UPGRADE PROCEDURE
Over Ethernet
- Ensure ISR-2/4 is connected to the same network as the PC using Integration Designer.
- Choose the "Update Firmware" command from the "Communications" menu in Integration Designer.
- Follow the instructions on screen to update your firmware.
- In the 'Select Update Method' window, select the ISR-2/4 that needs to be updated.
- Click Use Selected Device to send the firmware to the ISR-2/4.

Over USB-C
- Ensure ISR-2/4 is connected to the PC using Integration Designer with a USB-C cable.
- Choose the "Update Firmware" command from the "Communications" menu in Integration Designer.
- Follow the instructions on screen to update your firmware.
- In the 'Select Update Method' window, click Use USB connection to update firmware button.


LIST OF CHANGES IN THIS RELEASE 25.10.30
- Added Settings Reset button to the About page
- Fixed connection delays
- Fixed feedback issues when running a standalone macro
- Fixed page changes when using local macros
- Fixed issue where trigger commands don’t execute in a standalone macro
- Fixed scrolling text from preventing a layer being hidden
- Fixed URL redirects for dynamic images
- Fixed gateway showing as incorrect address
- Fixed occasional black background on viewports with visibility changes
- Fixed compatibility issues by disabling IPV6 addressing


LIST OF CHANGES IN RELEASE 25.06.20
- Added WiFi RSSI to control panel
- Added "Page Mode" support for viewports
- Added support for button "line" attributes (width, color)
- Added Arabic fonts
- Updated system sounds to be played via macros.
- Updated support for large sounds and images
- Fixed Page Link > Previous not being added to history
- Fixed Allow Images setting for lists
- Fixed standalone IR.
- Fixed dynamic images becoming blurry over time as they changed
- Fixed text animations - now stop after 3 cycles
- Fixed thumb size to no longer scale with slider
- Fixed macros that set local flags
