RTI IST-5 and IST-10 Firmware Version 26.3.17

PREREQUISITES FOR USING THIS UPGRADE PROCEDURE
Integration Designer 11.10.2 or higher must already be installed on the PC 
that you wish to use to upgrade the IST firmware.

FIRMWARE UPGRADE PROCEDURE
Over Ethernet
- Ensure IST-5 or IST-10 is connected to the same network as the PC using Integration Designer.
- Choose the "Update Firmware" command from the "Communications" menu in Integration Designer.
- Follow the instructions on screen to update your firmware.
- In the 'Select Update Method' window, select the IST-5 or IST-10 that needs to be updated.
- Click Use Selected Device to send the firmware to the IST-5 or IST-10.

LIST OF CHANGES IN THIS RELEASE (RELEASE 26.3.17)
- Added the Advanced Web Object
- Video engine changed to VLC
- Added Viewport Frame Indicators
- Added Ringtone selection including custom ringtone to settings screen (Requires ID11.14 or newer)
- Added Call/Ring Volume controls to settings screen

LIST OF CHANGES IN RELEASE 25.11.21
- Fixed crash resulting in “IST RTiPanel Not Responding” popup on screen
- Fixed issue with IST stuck in continual loop between light and dark screen
- Fixed backlight active and idle not working
- Fixed proximity sensor operation issues
- Fixed issues relating to multiple RTSP feeds on the same page in Layers or Viewport
- Fixed screen timeout default
- Fixed ID Power Down Time/Screen Timeout setting not working
- Fixed the MAC address missing on the settings screen
- Fixed status to show correct information in ID during IST communication

LIST OF CHANGES IN RELEASE 24.10.17
- Added support for setting static IP addresses from Integration Designer for both Wi-Fi and Ethernet configurations.
- Updated camera’s aspect ratio.
- Added Forget button when connected to an SSID.
- Enhanced ALS and proximity sensor logic.
- Fixed FW updates when the internet is not detected.